Arlington Heights School District 25 **Food Service Equipment Bid Form**

Patton Elementary School

| **#** | **Item** | **Manufacturer** | **Model/Specifications** | **Qty** | **Per Unit Bid (Net)** | **Total Cost (Net Total)** |
| --- | --- | --- | --- | --- | --- | --- |
| 1 | Milk Cooler, Dual Access | Continental, Norlake, True or Approved Alternate\* | [Continental Model MC3NDCW](https://drive.google.com/file/d/12d4cvRpzkWGAe1csuJt84azhXeDZT3zz/view?usp=sharing) - 34” Dual Access Milk Cooler, White and Stainless Steel Exterior, Stainless Steel interior[Norlake Model NLMC08DW -](https://drive.google.com/file/d/1DEdzPwLOkOl52g6EFPR8hRyaLL-urwxa/view?usp=sharing) 34” Dual Access Milk Cooler, White and Stainless Steel Exterior, Stainless Steel interior[True Model TMC-34-DS-SS-HC](https://drive.google.com/file/d/1fldCh4vfA2f5kr3rDLdE0SJgd9IQdEd2/view?usp=sharing) - 34” Dual Sided Milk Cooler, White and Stainless Steel Exterior, Stainless Steel interior | 1 |  |  |
| 1a | Milk Cooler, Dual Access (Alternate) |  |  |  |  |  |
| 2 | Milk Cooler, Single Access | Continental, Norlake, True or Approved Alternate\* | [Continental Model MC3NSCW](https://drive.google.com/file/d/1HbcgAH41cvLAevxi0nLZnI_9t0-2mhWP/view?usp=drive_link) - 34” Milk Cooler, White and Stainless Steel Exterior, Stainless Steel interior[Norlake Model NLMC08SW](https://drive.google.com/file/d/1Po5lVRETfTR4GW2iklhwxMlBQImwP_07/view?usp=sharing) - 34” Milk Cooler, White and Stainless Steel Exterior, Stainless Steel interior[True Model TMC-34-SS-HC](https://drive.google.com/file/d/1sLr3jck06iygUAbfPOWU0CW9A2RxQe8E/view?usp=sharing) - 34” Milk Cooler, White and Stainless Steel Exterior, Stainless Steel interior | 1 |  |  |
| 2a | Milk Cooler, Single Access (Alternate) |  |  |  |  |  |
| 3 | Reach In Cooler | True or Approved Alternate\* | [True Mfg. ‐ General Foodservice Model No. TS‐72‐HC](https://drive.google.com/file/d/1aitMnigWuJfg6HcMd3qujtDTERowxrAx/view?usp=sharing)Refrigerator, reach‐in, three‐section, (3) stainless steel doors, (9) gray PVC coated adjustable wire shelves, interior lighting, stainless steel front/sides, stainless steel interior, 4" castors, R290 Hydrocarbonrefrigerant, 3/4 HP, 115v/60/1‐ph, 6.9 amps, NEMA 5‐15P, cULus, UL, EPH Classified, Made in USA* 1 ea Self‐contained refrigeration standard
* 1 ea 7 year compressor warranty, 6 years parts warranty, 5 year labor warranty standard.
* 1 ea Left door hinged left, center & right doors hinged right, standard
* 1 ea 4" stem castors, standard (adds 5" to OA height)
 | 1 |  |  |
| 3a | Reach In Cooler (Alternate) |  |  |  |  |  |
| 4 | Reach In Freezer | True or Approved Alternate\* | [True Mfg. ‐ General Foodservice Model No. T-19FZ-HC](https://drive.google.com/file/d/1U2wIt_XQ8blIseom2kOIf_rggXsq7Emp/view?usp=sharing)Reach-in solid swing door, 0 degrees Freezer with Hydrocarbon Refrigerant,PVC coated adjustable wire shelves, interior lighting, stainless steel front/sides, stainless steel interior, 4" castors, R290 Hydrocarbon refrigerant, 3/4 HP, 115v/60/1‐ph, 6.9 amps, NEMA 5‐15P, cULus, UL, EPH Classified, Made in USA* 1 ea 7 year compressor warranty, 6 years parts warranty, 5 year labor
* 1 ea 4" stem castors, standard (adds 5" to OA height)
 | 1 |  |  |
| 4a | Reach In Freezer (Alternate) |  |  |  |  |  |
| 5 | Work Table w/ Undershelf | John Boos, Eagle or Approved Alternate\* | [16 GA Stainless Steel Top Work Table](https://drive.google.com/file/d/1cIZbyVDlHHSluOh4mRTjTiIZxGnjYXn3/view?usp=sharing) 72” w/ backsplash, Stainless Steel Legs, and adjustable undershelf. Adjustable Stainless feet | 1 |  |  |
| 5a | Work Table w/ Undershelf (Alternate) |  |  |  |  |  |
| 6 | Serving Counter, Frost Top | Randell, LTI or Approved Alternate\*  | [Randell Model No. RS SSC-RFT-2](https://drive.google.com/file/d/14dkSQJBELIme4Wumh9uii_4WaoA_GbdS/view?usp=sharing) Frost Top Unit, 36"W x 30"D x 35-1/2"H, mobile modular, enclosed base, 16 gauge stainless steel top, laminate exterior with galvanized backing, 1/4 HP* (1) year parts and labor warranty, standard
* CW5 5 yr. compressor warranty (NET)
* 115v/60/1-ph, 3.5 amps, NEMA 5-15P
* RSHGTMOD Elementary Counter, school height (30-1/2" work height)
* RSEXTLAM-36 Laminate Exterior (specify color), for 36" units
* RAN SBS36 Single Sided Buffet Shield, 36"W, stainless steel top, acrylic insert
* RAN INV36-C Inverted "V" Tray Slide, 10" deep, customer side
* 6" swivel casters (2 locking), standard
* RSKCKPLT36 Kick/Toe Plate, for 36" RanServe units, laminate or stainless
 | 1 |  |  |
| 6a | Serving Counter, Frost Top (Alternate) |  |  |  |  |  |
| 7 | Serving Counter, Cold Food | Randell, LTI or Approved Alternate\*  | [Randell Model No. RS SSC-RCP-3](https://drive.google.com/file/d/19cgoUNAeXV_4SzypWRphw8_frY6OSLC-/view?usp=sharing) Cold Food Table, 48"W x 30"D x 35-1/2"H, mobile modular, self-contained refrigeration, (3) 12" x 20" pan capacity, 16 gauge stainless steel top, electronic controls, enclosed base, stainless steel interior & exterior, (4) swivel casters (2 locking), 1/4 HP, NSF, cUL, UL, Made in USA* (1) year parts and labor warranty, standard
* CW5 5 yr. compressor warranty (NET)
* 115v/60/1-ph, 3.5 amps, NEMA 5-15P, standard
* RSHGTMOD Elementary Counter, school height (30-1/2" work height)
* RSEXTLAM-48 Laminate Exterior (specify color), for 48" units
* RAN SBS48 Single Sided Buffet Shield, 48"W, stainless steel top, acrylic insert
* RAN INV48-C Inverted "V" Tray Slide, 10" deep, customer side
* 6" swivel casters (2 locking), standard
* RSKCKPLT48 Kick/Toe Plate, for 48" RanServe units, laminate or stainless
 | 1 |  |  |
| 7a | Serving Counter, Cold Food (Alternate) |  |  |  |  |  |
| 8 | Hot Food Serving Counter | Randell, LTI or Approved Alternate\*  | [Model No. RAN HTD-3](https://drive.google.com/file/d/1EZ6EBbGSazguHTMG0V0djJvRZGWLgxv6/view?usp=sharing), Hot Food Table, electric, 48"W x 30"D x 35-1/2"H, mobile modular, (3) 12" x 20" hot food wells with individual thermostatic controls, enclosed cabinet base, 16 gauge stainless steel top, laminate exterior with galvanized backing, (4) swivel casters (2 with brakes), cULus, NSF, Made in USA* (1) year parts and labor warranty, standard
* Note: Amperage for base unit only. Any accessory heat lamp or display illumination loads must be added to the total amperage
* 120v/60/1-ph, 12.50 amps, 500 watts, NEMA 5-20P
* RSEXTLAM-48 Laminate Exterior (specify color), for 48" units
* RAN CP48-GL Counter Protector, for 48" units, with glass top
* HLINST-HL Heat Lamp, by others, installation charge
* RSPREWIR Prewire Unit
* RAN INV48-C Inverted "V" Tray Slide, 10" deep, customer side
* 6" swivel casters (2 locking), standard
* RSKCKPLT48 Kick/Toe Plate, for 48" RanServe units, laminate or stainless
 | 1 |  |  |
| 8a | Hot Food Serving Counter (Alternate) |  |  |  |  |  |
| 9 | Serving Counter, Utility | Randell, LTI or Approved Alternate\*  | [Model No. RAN ST-3](https://drive.google.com/file/d/1HLGpCFh4n6ukNG_9hFQOusQuntQdeVxN/view?usp=sharing) , Utility Unit, 36"W x 30"D x 35-1/2"H, mobile modular, enclosed base, 16 gauge stainless steel top, laminate exterior with galvanized backing, NSF, Made in USA* (1) year parts and labor warranty, standard
* RSHGTMOD Elementary Counter, school height (30-1/2" work height)
* RSEXTLAM-36 Laminate Exterior (specify color), for 36" units
* RAN SBS36 Single Sided Buffet Shield, 36"W, stainless steel top, acrylic insert
* RAN INV36-C Inverted "V" Tray Slide, 10" deep, customer side
* 6" swivel casters (2 locking), standard
* RSKCKPLT36 Kick/Toe Plate, for 36" RanServe units, laminate or stainless
 | 1 |  |  |
| 9a | Serving Counter, Utility (Alternate) |  |  |  |  |  |
| 10 | Cash Stand Register | Randell, LTI or Approved Alternate\* | [Model No. RAN CA](https://drive.google.com/file/d/1TYxOCOFd0Meo6o7fbQhTa2U39pWPfq5z/view?usp=sharing), Cash Register Stand, 30"W x 30"D x 35-1/2"H, mobile modular, with locking cash drawer, foot rest & cash register cord hole, 16 gauge stainless steel top with interchangeable laminate body panels, swivel casters (2 locking)* (1) year parts and labor warranty, standard
* RSHGTMOD Elementary Counter, school height (30-1/2" work height)
* RSEXTLAM-CA Laminate Exterior (specify color)
* RAN INV30-S Inverted "V" Tray Slide, 10" deep, server side
* 6" Casters, standard
* RSKCKPLT30 Kick/Toe Plate, for 30" RanServe units, laminate or stainless
 | 1 |  |  |
| 10a | Cash Stand Register (Alternate) |  |  |  |  |  |
| 11 | Flatware and Tray Cart | Randell, LTI or Approved Alternate\* | [Model No. RAN SW-8](https://drive.google.com/file/d/1GXZlwJb8Dsp1oPZoTADmuxVcIu_vD2FC/view?usp=sharing), Tray & Silverware Dispenser, 30"W x 30"D x 35"H, mobile modular, enclosed design, eight-hole silverware holder, stainless steel shelf area for tray stacking, 16 gauge stainless steel top with plastic laminate panels, swivel casters (2 locking), NSF, Made in USA* (1) year parts and labor warranty, standard
* RSEXTLAM-SW8 Laminate Exterior (specify color)
* 6" swivel casters (2 locking), standard
* RSKCKPLT30 Kick/Toe Plate, for 30" RanServe units, laminate or stainless
 | 1 |  |  |
| 11a | Flatware and Tray Cart (Alternate) |  |  |  |  |  |
| Total Equipment Cost: |  |
| Total Install Cost:  |  |

\*If bidding an alternate, please specify manufacturer, model number and specifications (including warranty information) in the space provided. Please also attach spec sheets.

Delivery & Install Information:

Patton Elementary School

1616 N. Patton Ave.

Arlington Heights, IL 60004
No Dock - lift gate needed

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name and Title of Person Authorizing this Bid:

Company Name:

Authorized Signature:

Date: